How to use the loader

1. Turn off the electronic unit (if it was on). The unit should be connected to the host PC by USB cable.
2. Wait for 30-60 second (for capacitors discharge).
3. Press and hold pressed 'UP' button on the front panel of the electronic unit, turn the electronic unit on. You will enter the bootloader mode of the unit.
4. On host PC, start program load.exe
5. Pressing button 'File' in the program, select file 'LB_bath.bin'.
6. In selector 'Select serial port' choose corresponding serial port for connection with the electronic unit.
7. 
	>>> Prepare to load the firmware into the unit: during following operation please do not work with host PC (don't type or move mouse better, the PC should be busy with the uploading only during that) <<<
Press button 'Upload firmware' in the loader program. Wait till the firmware uploading finishes. After correct uploading, you will get notification 'Firmware loaded!'
8. After upload finishes, close loader program and run the LB control software to check the dipper motions.

<Russian>
Выключить устройство.
Подождать 30 сек.
Зажать кнопку "вверх" на блоке электроники и, удерживая эту кнопку, включить питание блока.
В программе: load открыть файл LB_bath.bin (кнопка File).
Выбрать последовательный порт Select serial port.
Нажать на кнопку "Upload firmware".
!!!ВАЖНО!!! - Не трогать компьютер пока не будет залита прошивка полностью.
Ждать до появления сообщения Firmware loaded!
Либо другое сообщение, но это будет некорректная заливка.
